FM173

Looking at the Restart states from Rev 174 we have the following results for FM173.

FM139	 	NoBurn	Plan 	OD 	Plan-NoBurn	OD-NoBurn	Plan-OD	error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (m)	 	
MMS1	Sep 02 2015 16:47:42.993	42100.033	42109.316	42109.340	9.282	9.307	-24.712	-0.27%	
MMS2	Sep 02 2015 16:48:20.540	42112.808	42109.329	42109.318	-3.480	-3.490	10.334	-0.30%	
MMS3	Sep 02 2015 16:49:22.036	42102.342	42109.354	42109.330	7.012	6.988	24.016	0.34%	

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs 
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
The predicted velocity meets all requirements with significant margin.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Reg. (m/s)/
DiffVZ(m/s)	
MMS1_FM173	244/14:46:30 - 244/14:49:00	-0.129011	-0.661414	-1.231197	
		0.002	0.0066	0.012	
		0.00005	0.00005	0.00002	
MMS2_FM173	244/17:58:00 - 244/17:59:00	-0.255030	0.706134	0.131984	
		0.0025	0.007	0.002	
		0.0002	0.0001	0.00005	
MMS3_FM173	244/16:21:40 –
244/16:24:00	-0.020231	-0.776901	-1.20476	
		0.002	0.0077	0.012	
		0.0012	0.0011	0.0005