FR217

Looking at the Restart states from Rev 218 we have the following results for FR217. 

FR202		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)		
MMS1	Oct 16 2015 11:54:46.565	42117.497	42113.344	42113.285	-4.154	-4.212	-0.05850	1.41%	
MMS2	Oct 16 2015 11:54:52.210	42102.823	42113.353	42113.275	10.529	10.452	-0.07732	-0.73%	
MMS4	Oct 16 2015 11:54:46.649	42103.275	42113.319	42113.265	10.044	9.990	-0.05376	-0.54%	

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated maneuver planning requirements for 1 orbit predictions for FR217
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time, starting with the post-perigee GEONS state from the previous perigee for FR217 vs the definitive GEONS state at the time of the maneuver.
The predicted velocity differences at the time of each maneuver are less than the greater of 1% of the delta-V or 2 mm/s for the second maneuver with significant margin.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS4_FR217	288/08:10:50- 288/08:14:00	-0.251538	-0.355848	-1.325933	
		0.0025	0.0035	0.013	
		<0.001	<0.001	<0.001	
MMS2_FR217	288/09:30:20- 288/09:34:00	-1.520205	-2.006581	-0.863092	
		0.015	0.020	0.0086	
		<0.001	<0.001	<0.001	
MMS1_FR217	288/14:27:50–
288/14:29:00	-0.393095	-0.181987	-0.539993	
		0.004	0.002	0.005	
		<0.001	<0.001	<0.001	

All FR217 maneuvers were originally planned using predicted ephemeris files based on GEONS post-perigee RST vectors @ 2015-285/02:56, one day prior to the CAM.  Note that these predictions start 3+ orbits prior to FR217.  Because the FR216 maneuvers started only a couple of hours post-perigee,  the CAM was held the prior day and final maneuver plans had to be prepared prior to the CAM. A “tweak” was planned for FR217 but decision was made to use the original plan. 
The Plan numbers above are the value from not changing the original plan but using the new RST vectors between maneuvers.  The original Plan SMA targets were ~ 42113.302 km which were closer to the Rev 218 OD results than the Plan values from the new RST vectors.