GS802

Looking at the Restart states from Rev 803 we have the following results for GS802.
GS802		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)		
MMS1	Oct 04 2017 13:09:45.481	83867.630	84199.409	84199.501	331.779	331.871	-0.09164	-0.028%	
MMS2	Oct 04 2017 13:09:00.592	83867.567	84196.768	84196.880	329.202	329.313	-0.11167	-0.034%	
MMS3	Oct 04 2017 13:08:17.899	83867.553	84194.069	84194.112	326.515	326.559	-0.04357	-0.013%	
MMS4	Oct 04 2017 13:07:41.606	83867.609	84191.496	84191.498	323.887	323.890	-0.00224	-0.001%	
		PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	dPH error	
MMS1	Oct 05 2017 22:55:30.544	1831.926	2508.936	2509.070	677.010	677.144	-0.13397	-0.020%	
MMS2	Oct 05 2017 22:54:39.743	1822.131	2489.422	2489.563	667.291	667.432	-0.14080	-0.021%	
MMS3	Oct 05 2017 22:53:51.032	1822.394	2480.722	2480.748	658.329	658.355	-0.02604	-0.004%	
MMS4	Oct 05 2017 22:53:09.031	1830.111	2481.093	2481.179	650.983	651.068	-0.08574	-0.013%	
 
MMS1 was 19.0 m/s and 16.8% axial, MMS2 was 18.70 m/s and 16.8% axial, MMS3 was 18.48 m/s and 17.3%axial, and MMS4 was 18.4 m/s and 17.6% axial.   

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_GS802	2017_274/15:02:57 to 2017_274/15:31:37	16.8659	5.6418	6.7493	
		0.16866	0.056418	0.067493	
		-0.002061	-0.001127	-0.0004601	
MMS2_GS802	2017_274/16:58:17 to 2017_274/17:26:37	16.5975	5.4971	6.6278	
		0.16598	0.054971	0.066278	
		-0.001866	-0.001426	-0.0006527	
MMS3_GS802	2017_274/18:53:37 to 2017_274/19:21:37	16.4308	5.346	6.5359	
		0.16431	0.05346	0.065359	
		-0.003223	0.0008295	-0.0004761	
MMS4_GS802	2017_274/20:49:27 to 2017_274/21:16:37	16.3837	5.2105	6.4874	
		0.16384	0.052105	0.064874	
		-0.001947	-0.001706	-0.0006325