FM868

Looking at the Restart states from Rev 869 we have the following results for FM868. AH = apogee height
FM868		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	Plane change error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Apr 08 2018 10:49:12.598	84267.826	84267.794	84267.799	-0.032	-0.027	-0.00529			
MMS2	Apr 08 2018 10:49:11.890	84261.376	84267.807	84267.828	6.431	6.452	-0.02047	-0.318%	0.719%	
MMS3	Apr 08 2018 10:49:25.674	84268.058	84267.801	84267.796	-0.257	-0.262	0.00553	-2.157%	0.426%	
MMS4	Apr 08 2018 10:49:28.125	84266.269	84267.801	84267.806	1.532	1.537	-0.00497	-0.324%	1.792%	
MMS	Epoch of Plan Apogee	AH (km)	AH (km)	AH (km)	AH (km)	AH (km)	AH (km)	AH error		
MMS1	Apr 08 2018 10:49:12.598	153990.086	153990.044	153989.990	-0.042	-0.096	0.05468			
MMS2	Apr 08 2018 10:49:11.890	153979.337	153977.884	153977.876	-1.453	-1.461	0.00805	-0.554%		
MMS3	Apr 08 2018 10:49:25.674	153991.621	153983.467	153983.391	-8.154	-8.230	0.07620	-0.935%		
MMS4	Apr 08 2018 10:49:28.125	153984.686	153983.412	153983.356	-1.273	-1.330	0.05675	-4.457%		
 
MMS2 was 0.048m/s (net delta-v) and 4.20% axial, MMS3 was 0.50 m/s and 31.56% axial, and MMS4 was 0.16 m/s and 7.60% axial.
Small SMA changes (MMS3) lead to large % errors.  MMS3 had a larger apogee height change and a low error there as well as with plane change. MMS4 for this maneuver had a small SMA error.

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement except MMS4 DVY  
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS2_FM868	2018_95/17:13:57 to 2018_95/17:14:37	0.4773	0.0051	-0.0376	
		0.004773	0.002	0.002	
		-0.0003859	0.00189	-0.0001346	
MMS4_FM868	2018_95/19:04:27 to 2018_95/19:04:37	0.16	-0.0206	-0.0055	
		0.002	0.002	0.002	
		-0.0006537	0.002857	-0.00006596	
MMS3_FM868	2018_95/22:43:57 to 2018_95/22:44:37	0.4009	-0.1108	-0.2687	
		0.004009	0.002	0.002687	
		0.000161	0.0016	0.0001298