AR975

Looking at the Restart states from Rev 977 we have the following results for AR975
AR975		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	Plane change error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Feb 07 2019 04:55:48.182	84256.897	91610.484	91612.647	7353.587	7355.750	-2.16267	-0.029%	0.095%	
MMS2	Feb 07 2019 04:53:49.084	84257.087	91609.361	91610.721	7352.274	7353.633	-1.35945	-0.018%	0.090%	
MMS3	Feb 07 2019 05:00:28.662	84256.886	91609.250	91611.012	7352.364	7354.127	-1.76252	-0.024%	0.105%	
MMS4	Feb 07 2019 04:57:03.996	84256.861	91609.306	91614.266	7352.445	7357.405	-4.96077	-0.067%	0.178%	
MMS	Epoch of Plan Apogee	Period (min)	Period (min)	Period (min)	Period (min)	Period (min)	Period (min)	OD P (hrs)		
MMS1	Feb 07 2019 04:55:48.182	4056.654	4599.149	4599.312	542.496	542.658	-0.16286	76.6552		
MMS2	Feb 07 2019 04:53:49.084	4056.667	4599.065	4599.167	542.397	542.500	-0.10237	76.65278		
MMS3	Feb 07 2019 05:00:28.662	4056.653	4599.056	4599.189	542.403	542.536	-0.13273	76.65315		
MMS4	Feb 07 2019 04:57:03.996	4056.651	4599.060	4599.434	542.409	542.783	-0.37357	76.65723		
 
MMS1 was 19.78 m/s (net delta-v) and 0.67% axial, MMS2 was 19.78 m/s (net delta-v) and 0.66% axial, MMS3 was 19.78 m/s and 0.86% axial, and MMS4 was 19.78 m/s and 0.72% axial.
  
The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft do meet the requirement, except for DVY for all MMS, and DVX for MMS3, 
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_AR975	2019_33/09:30:00 to 2019_33/10:02:30	-16.4969	-10.2379	-3.8184	
		0.164969	0.102379	0.038184	
		0.1365	0.3157	-0.006687	
MMS2_AR975	2019_33/09:28:10 to 2019_33/10:00:30	-16.4931	-10.2429	-3.8163	
		0.164931	0.102429	0.038163	
		0.100	0.2333	-0.00368	
MMS3_AR975	2019_33/09:34:50 to 2019_33/10:07:10	-16.5075	-10.2204	-3.8049	
		0.165075	0.102204	0.038049	
		0.3104	0.6228	-0.00313	
MMS4_AR975	2019_33/09:31:40 to 2019_33/10:03:30	-16.5148	-10.2127	-3.804	
		0.165148	0.102127	0.03804	
		0.1418	0.3771	-0.006754