PR014 Goals and CHiFi

Desired SMA 42093.3745 km

Nominal Plan (not scaled back)

MMS 1 No Burn Next Rev Apogee    --> SMA [km] 41982.8496
MMS 1 With Burn Next Rev Apogee  --> SMA [km] 42093.0284
Delta-SMA = 110.1788 km

MMS 2 No Burn Next Rev Apogee    --> SMA [km] 41983.2627
MMS 2 With Burn Next Rev Apogee  --> SMA [km] 42093.2802
Delta-SMA = 110.0175 km

MMS 3 No Burn Next Rev Apogee    --> SMA [km] 41984.2810
MMS 3 With Burn Next Rev Apogee  --> SMA [km] 42093.3954
Delta-SMA =  109.1144 km

MMS 4 No Burn Next Rev Apogee    --> SMA [km] 41985.1798
MMS 4 With Burn Next Rev Apogee  --> SMA [km] 42093.5713
Delta-SMA = 108.3915 km
-----------------------------------------------

Recon from AMS
Scaled Plan on S/C

DOY 87 apogee:
MMS1  From OD:  42093.0536 km
      Recon: 	42092.9926 km	
      Plan: 	42093.0284 km	
   Scaled Plan: 42086.1078 km

(period difference OD -Plan 0.08 secs)

MMS2  From OD: 	42093.3283 km
      Recon: 	42093.2287 km
	 Plan: 	42093.2802 km
   Scaled Plan: 42086.3294 km

(period difference OD  - Plan 0.15 seconds)

MMS3  From OD: 	42094.4684 km	
	 Recon: 	42094.4364 km
	Plan: 	42093.3954 km 
   Scaled Plan: 42086.4303 km

(period difference OD - Plan  3.29 seconds)

MMS4 From OD:	42094.9667 km
	Recon: 	42094.9761 km
	Plan: 	42093.5713 km 
   Scaled Plan: 42086.5893 km

(period difference OD - Plan 4.27 seconds)

PR014	No Burn	Scaled 	Plan 	Recon 	OD	
	SMA	SMA	SMA	SMA	SMA	
MMS1	41982.85	42086.11	42093.03	42092.99	42093.05	
MMS2	41983.26	42086.33	42093.28	42093.23	42093.33	
MMS3	41984.28	42086.43	42093.4	42094.44	42094.47	
MMS4	41985.18	42086.59	42093.57	42094.98	42094.97	
						
	Scaled	Plan 	Recon 	OD		
	Δ SMA	Δ SMA	Δ SMA	Δ SMA		
MMS1	103.2582	110.1788	110.143	110.204		
MMS2	103.0667	110.0175	109.966	110.0656		
MMS3	102.1493	109.1144	110.1554	110.1874		
MMS4	101.4095	108.3915	109.7963	109.7869		
						
	PR014 % hot to scaled	PR011 % hot to scaled	PR009 % hot to scaled	PR007 % hot		
						
MMS1	6.73	8.57	12.89	12.90		
MMS2	6.79	8.67	10.73	10.19		
MMS3	7.87	9.66	11.20	10.01		
MMS4	8.26	10.31	10.10	7.33		
						
	PR014 % hot to plan	PR011% hot to plan	PR009 % hot to plan	PR007 % hot		
						
MMS1	0.02	-0.24	5.71	12.90		
MMS2	0.04	-0.01	3.90	10.19		
MMS3	0.98	0.85	4.41	10.01		
MMS4	1.29	1.51	3.46	7.33