FM673

Looking at the Restart states from Rev 674 we have the following results for FM673.
FM673		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	dSMA error	PC error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jan 12 2017 07:26:59.382	42106.580	42102.032	42102.009	-4.54743	-4.57053	0.02310	-0.51%	0.90%	
MMS2	Jan 12 2017 07:26:55.424	42106.579	42106.662	42106.675	0.08330	0.09571	-0.01242	-14.91%	-0.25%	
MMS3	Jan 12 2017 07:26:56.359	42106.557	42106.557	42106.561	-0.00001	0.00331	-0.00332			
MMS4	Jan 12 2017 07:26:51.571	42106.580	42101.226	42101.221	-5.35366	-5.35850	0.00484	-0.09%	0.57%	
		AH(km)	AH(km)	AH(km)	AH(km)	AH(km)	AH(km)	dAH error		
MMS2	Jan 12 2017 07:26:55.424	70140.12294	70144.91809	70144.9487	4.79515	4.82576	-0.03061	-0.64%		

MMS1 was 0.339 m/s and 35.6% axial, MMS2 was 0.486 m/s and 2.27% axial, MMS4 was 0.829 m/s and 22.4% axial. The small SMA change for MMS2 above produced larger percentage error values in SMA error, but MMS2 had a large apogee height and perigee height change.  The apogee height error is more representative of how well MMS2 did.     

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan0	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS4_FM673	2017_011/10:01:12 to 2017_011/10:02:12	0.0005	-0.7903	-0.0946	
		0.01	0.01	0.01	
		-0.00057	0.0034	0.001	
MMS1_FM673	2017_011/13:11:12 to 2017_011/13:11:42	-0.0667	-0.243	-0.2151	
		0.01	0.01	0.01	
		-0.0018	0.0046	0.00077	
MMS2_FM673	2017_011/14:46:12 to 2017_011/14:46:52	-0.4841	0.053	0.0466	
		0.01	0.01	0.01	
		-0.0031	0.0055	0.00046