FM674

Looking at the Restart states from Rev 675 we have the following results for FM674.
FM674		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	PC error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jan 13 2017 07:20:12.002	42101.747	42106.231	42106.250	4.48364	4.50250	-0.01885	-0.42%	0.37%	
MMS2	Jan 13 2017 07:20:11.154	42106.413	42106.266	42106.266	-0.14765	-0.14695	-0.00071	0.48%	0.46%	
MMS3	Jan 13 2017 07:20:09.094	42106.299	42106.257	42106.256	-0.04237	-0.04297	0.00060			
MMS4	Jan 13 2017 07:20:14.254	42100.959	42106.228	42106.275	5.26898	5.31522	-0.04625	-0.88%	0.74%	
		AH(km)	AH(km)	AH(km)	AH(km)	AH(km)	AH(km)	dAH error		
MMS2	Jan 13 2017 07:20:11.154	70140.198	70142.114	70142.128	1.91633	1.93029	-0.01396	-0.73%		
 
MMS1 was 0.75 m/s and 12.7% axial, MMS2 was 0.24 m/s and 31% axial, MMS4 was 0.41 m/s 19.9% axial.   The MMS2 SMA change was almost twice for FM674 than FM673.  This time there was more agreement between the plan and the OD result.  The Apogee Height change is here for reference for MMS2.      

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS4_FM674	2017_012/01:19:07 to 2017_012/01:19:37	0.1102	-0.2374	-0.2821	
		0.002	0.002374	0.002821	
		-0.00018	0.000091	-0.00016	
MMS1_FM674	2017_012/02:48:37 to 2017_012/02:49:37	-0.2133	-0.6794	-0.2485	
		0.002133	0.006974	0.002485	
		-0.00044	-0.0009	-0.0005	
MMS2_FM674	2017_012/04:19:17 to 2017_012/04:19:37	-0.0785	-0.0094	-0.1278	
		0.002	0.002	0.002	
		-0.00023	0.00073	-0.00029