GS742

Looking at the Restart states from Rev 743 we have the following results for GS742.
GS742		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)		
MMS1	Apr 19 2017 12:32:02.369	83618.640	83875.528	83875.694	256.889	257.054	-0.16546	-0.064%	
MMS2	Apr 19 2017 12:14:55.953	83622.381	83906.440	83906.662	284.058	284.280	-0.22189	-0.078%	
MMS3	Apr 19 2017 12:00:42.158	83620.592	83942.585	83942.743	321.993	322.151	-0.15808	-0.049%	
MMS4	Apr 19 2017 11:56:41.269	83617.348	83963.262	83963.407	345.914	346.058	-0.14447	-0.042%	
		PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	dPH error	
MMS1	Apr 20 2017 22:08:39.148	1516.169	2034.984	2035.257	518.815	519.088	-0.27328	-0.053%	
MMS2	Apr 20 2017 21:52:39.940	1572.940	2143.727	2143.935	570.787	570.994	-0.20744	-0.036%	
MMS3	Apr 20 2017 21:39:44.774	1574.577	2217.190	2217.340	642.613	642.763	-0.14986	-0.023%	
MMS4	Apr 20 2017 21:36:28.748	1567.485	2256.737	2257.072	689.252	689.588	-0.33580	-0.049%	
 
MMS1 was 15.1 m/s and 32.0% axial, MMS2 was 16.37 m/s and 31.9% axial, MMS3 was 18.37 m/s and 32.3%axial, and MMS4 was 19.85 m/s and 32.6% axial.   

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_GS742	2017_106/13:04:57 to 2017_106/13:26:37	13.5143	2.5195	6.2815	
		0.135143	0.025195	0.062815	
		0.002005	0.002116	0.000407	
MMS2_GS742	2017_106/15:18:07 to 2017_106/15:41:37	14.6381	2.7357	6.7851	
		0.146381	0.027357	0.067851	
		0.002238	0.00204	0.002185	
MMS3_GS742	2017_106/18:35:07 to 2017_106/19:01:37	16.4495	2.982	7.6002	
		0.164495	0.02982	0.076002	
		0.001551	0.004341	0.001416	
MMS4_GS742	2017_106/20:48:47 to 2017_106/21:16:37	17.8015	3.1276	8.1999	
		0.178015	0.031276	0.081999	
		-0.00024	0.008466	0.003271