FR759

Looking at the Restart states from Rev 760 we have the following results for FR759.
FR759		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	PC Error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jun 06 2017 02:25:23.608	83900.748	83888.963	83888.825	-11.785	-11.923	0.13807	-1.172%	0.652%	
MMS2	Jun 06 2017 02:25:16.308	83894.845	83888.806	83888.732	-6.039	-6.112	0.07370	-1.220%	0.131%	
MMS3	Jun 06 2017 02:25:06.608	83888.869	83888.849	83888.839	-0.020	-0.030	0.01007			
MMS4	Jun 06 2017 02:24:56.782	83887.076	83888.793	83888.748	1.717	1.672	0.04448	2.591%	0.468%	
 
Looking at the Restart states from Rev 761 we have the following results for FR759.
FR759		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	PC Error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jun 08 2017 21:37:51.820	83930.563	83918.700	83918.578	-11.863	-11.985	0.12117	-1.021%	0.487%	
MMS2	Jun 08 2017 21:37:43.796	83924.641	83918.540	83918.492	-6.100	-6.149	0.04816	-0.790%	-0.068%	
MMS3	Jun 08 2017 21:37:34.359	83918.651	83918.594	83918.616	-0.057	-0.035	-0.02197			
MMS4	Jun 08 2017 21:37:24.308	83916.853	83918.538	83918.517	1.685	1.664	0.02110	1.252%	0.352%	

MMS1 was 0.70 m/s (net delta-v) and 4.07% axial, MMS2 was 0.48 m/s and 28.16% axial, and MMS4 was 0.23 m/s and 59.73% axial.   

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement 
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS2_FR759	2017_153/18:38:57 to 2017_153/18:39:37	0.1451	0.1142	0.2679	
		0.002	0.002	0.002679	
		-0.00008257	-0.0001089	0.000647	
MMS1_FR759	2017_153/20:28:57 to 2017_153/20:29:37	-0.0832	-0.2636	0.0983	
		0.002	0.002636	0.002	
		0.0002148	0.001007	0.0008975	
MMS4_FR759	2017_153/23:28:37 to 2017_153/23:29:37	-0.2226	0.5782	0.2407	
		0.002226	0.005782	0.002407	
		0.0004738	0.0007794	0.0003334