FM791

Looking at the Restart states from Rev 792 we have the following results for FM791.
FM791		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	PC Error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Sep 03 2017 17:39:58.203	83931.356	83934.096	83934.002	2.741	2.646	0.09413	3.435%	-0.686%	
MMS2	Sep 03 2017 17:39:53.487	83934.942	83934.077	83933.929	-0.865	-1.013	0.14756	-17.058%	-0.734%	
MMS3	Sep 03 2017 17:39:46.816	83934.421	83934.017	83933.881	-0.404	-0.540	0.13600	-33.659%	-3.988%	
MMS4	Sep 03 2017 17:39:37.919	83934.001	83933.978	83933.962	-0.023	-0.039	0.01573			
 
MMS1 was 0.15 m/s (net delta-v) and 8.27% axial, MMS2 was 0.11 m/s and 50.14% axial, and MMS43 was 0.11 m/s and 21.54% axial. 
Larger SMA % errors due to small size of the maneuver.  Error in terms of meters is in line with FR754 and FR769 previous maneuvers, but smaller maneuvers. Note that errors cancel out part of FM790 for each MMS.

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement except all DVX, MMS3 DVY and MMS1 DVY.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS2_FM791	2017_243/06:59:17 to 2017_243/06:59:37	-0.0602	0.016	-0.1004	
		0.002	0.002	0.002	
		0.004509	-0.001276	0.001455	
MMS3_FM791	2017_243/10:29:27 to 2017_243/10:29:37	-0.083	-0.0435	-0.0673	
		0.002	0.002	0.002	
		0.003672	-0.005783	0.0003237	
MMS1_FM791	2017_243/12:19:27 to 2017_243/12:19:37	0.0117	-0.1459	-0.0506	
		0.002	0.002	0.002	
		0.003651	-0.00232	0.001249