FR972

Looking at the Restart states from Rev 972 we have the following results for FR972
FR972		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	Plane change error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jan 26 2019 08:47:30.564	84232.718	84249.284	84249.301	16.567	16.583	-0.01622	-0.098%	104.51%	
MMS2	Jan 26 2019 08:47:39.753	84232.704	84268.288	84268.342	35.583	35.638	-0.05448	-0.153%	-0.271%	
MMS3	Jan 26 2019 08:46:58.685	84232.714	84197.709	84197.712	-35.005	-35.002	-0.00247	0.007%	0.009%	
MMS4	Jan 26 2019 08:46:47.109	84232.725	84216.382	84216.306	-16.343	-16.419	0.07640	-0.467%	-0.103%	
 
MMS1 was 0.386 m/s (net delta-v) and 14.74% axial, MMS2 was 1.59 m/s (net delta-v) and 17.62% axial , MMS3 was 2.70 m/s and 7.32% axial, and MMS4 was 0.819 m/s and 17.68% axial.
The plane change for MMS1 was a factor of ~400 smaller than the other spacecraft (very, very small), which is why the error percentage was so large.  
The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement except MMS1 DVx , and MMS1 DVy.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS3_FR972	2019_024/05:16:12 to 2019_024/05:20:22	2.6941	-0.1759	-0.0171	
		0.026941	0.01	0.01	
		0.004344	-0.00576	0.001052	
MMS4_FR972	2019_024/09:46:12 to 2019_024/09:47:22	0.8076	0.0188	0.1331	
		0.01	0.01	0.01	
		0.00276	-0.004339	-0.0004725	
MMS2_FR972	2019_024/11:21:12 to 2019_024/11:23:42	-1.5505	-0.119	0.3101	
		0.015505	0.01	0.01	
		0.002616	-0.004361	0.000342	
MMS1_FR972	2019_024/17:56:12 to 2019_024/17:56:42	-0.3705	-0.101	0.028	
		0.01	0.01	0.01	
		0.01649	-0.01083	-0.0004472