FR973

Looking at the Restart states from Rev 974 we have the following results for FR973
FR973		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	Plane change error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jan 29 2019 04:21:43.928	84235.972	84219.402	84219.403	-16.569	-16.569	-0.00054	0.003%	-55.953%	
MMS2	Jan 29 2019 04:19:50.693	84255.001	84219.413	84219.568	-35.589	-35.433	-0.15533	0.436%	0.792%	
MMS3	Jan 29 2019 04:26:30.927	84184.410	84219.380	84219.435	34.970	35.024	-0.05440	-0.156%	-0.124%	
MMS4	Jan 29 2019 04:23:07.217	84202.993	84219.312	84219.373	16.319	16.379	-0.06019	-0.369%	0.369%	
 
MMS1 was 0.647 m/s (net delta-v) and 34.87% axial, MMS2 was 2.48 m/s (net delta-v) and 39.35% axial, MMS3 was 4.08 m/s and 34.99% axial, and MMS4 was 1.04 m/s and 29.17% axial.
The plane change for MMS1 was a factor of ~100 smaller than the other spacecraft (very small), which is why the error percentage was so large.  
The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_FR973	2019_025/17:43:37 to 2019_025/17:44:37	-0.1897	0.6175	0.0048	
		0.002	0.006175	0.002	
		0.00001098	0.0004669	-0.00000708	
MMS4_FR973	2019_025/19:33:07 to 2019_025/19:34:37	0.0869	-1.0295	-0.1258	
		0.002	0.010295	0.002	
		0.0001032	-0.0002899	-0.0001751	
MMS2_FR973	2019_025/21:20:07 to 2019_025/21:24:37	-0.4825	2.431	-0.1163	
		0.002	0.02431	0.002	
		0.00001273	0.00002823	-0.0002489	
MMS3_FR973	2019_025/23:08:27 to 2019_025/23:14:37	0.4254	-4.0596	-0.1288	
		0.002	0.040596	0.002	
		0.001863	-0.002031	-0.0003094