AR977

Looking at the Restart states from Rev 979 we have the following results for AR977
AR977		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	Plane change error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Feb 14 2019 01:20:32.816	91598.223	97410.707	97412.299	5812.483	5814.076	-1.59242	-0.027%	-0.055%	
MMS2	Feb 14 2019 01:18:23.803	91596.252	97410.686	97412.050	5814.434	5815.798	-1.36390	-0.023%	1.149%	
MMS3	Feb 14 2019 01:25:07.091	91596.690	97410.779	97412.824	5814.088	5816.134	-2.04566	-0.035%	1.098%	
MMS4	Feb 14 2019 01:22:10.203	91599.881	97410.552	97414.378	5810.671	5814.497	-3.82656	-0.066%	-0.055%	
MMS	Epoch of Plan Apogee	Period (min)	Period (min)	Period (min)	Period (min)	Period (min)	Period (min)	OD P (hrs)		
MMS1	Feb 14 2019 01:20:32.816	4598.226	5042.777	5042.901	444.551	444.675	-0.12366	84.04835		
MMS2	Feb 14 2019 01:18:23.803	4598.077	5042.775	5042.881	444.698	444.804	-0.10591	84.04802		
MMS3	Feb 14 2019 01:25:07.091	4598.110	5042.783	5042.942	444.672	444.831	-0.15885	84.04903		
MMS4	Feb 14 2019 01:22:10.203	4598.351	5042.765	5043.062	444.414	444.711	-0.29714	84.05104		
 
MMS1 was 13.81 m/s (net delta-v) and 0.80% axial, MMS2 was 13.81 m/s (net delta-v) and 0.71% axial, MMS3 was 13.81 m/s and 0.88% axial, and MMS4 was 13.81 m/s and 0.77% axial.
  
The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft do meet the requirement, except for DVY for all MMS, and DVX for MMS3, 
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_AR977	2019_39/19:07:50 to 2019_39/19:29:50	-11.5106	-7.1549	-2.6772	
		0.115106	0.071549	0.026772	
		0.0591	0.4207	-0.00373	
MMS2_AR977	2019_39/19:05:40 to 2019_39/19:27:40	-11.5501	-7.0961	-2.6489	
		0.115501	0.070961	0.026489	
		0.06652	0.3081	-0.001055	
MMS3_AR977	2019_39/19:12:20 to 2019_39/19:34:20	-11.5518	-7.0929	-2.6536	
		0.115518	0.070929	0.026536	
		0.04526	0.2009	-0.00009062	
MMS4_AR977	2019_39/19:09:10 to 2019_39/19:30:50	-11.5355	-7.1203	-2.6596	
		0.115355	0.071203	0.026596	
		0.1311	0.4804	-0.005701