GS1470

Looking at the Restart states from Rev 1471 we have the following results for GS1470.
GS1470		NoBurn	Plan	OD	Plan-NoBurn	OD-NoBurn	Plan-OD	SMA error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)		
MMS1	Nov 05 2023 06:45:54.037	97397.645	97748.699	97748.833	351.054	351.188	-0.13381	-0.038%	
MMS2	Nov 05 2023 06:46:37.113	97397.483	97750.766	97751.203	353.283	353.720	-0.43672	-0.124%	
MMS3	Nov 05 2023 06:48:09.013	97397.549	97755.430	97755.537	357.881	357.988	-0.10663	-0.030%	
MMS4	Nov 05 2023 06:47:17.238	97397.484	97753.037	97753.407	355.552	355.922	-0.36986	-0.104%	
		PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	PH(km)	dPH error	
MMS1	Nov 07 2023 01:01:16.058	1590.408	2295.309	2295.465	704.901	705.057	-0.15620	-0.022%	
MMS2	Nov 07 2023 01:02:03.989	1574.888	2287.588	2287.922	712.701	713.035	-0.33392	-0.047%	
MMS3	Nov 07 2023 01:03:46.806	1593.166	2321.542	2321.622	728.376	728.456	-0.07940	-0.011%	
MMS4	Nov 07 2023 01:02:49.398	1588.462	2308.847	2309.124	720.385	720.662	-0.27697	-0.038%	
 
MMS1 was 17.38 m/s and 10.35% axial, MMS2 was 17.70 m/s and 10.06% axial, MMS3 was 18.45 m/s and 10.41%axial, and MMS4 was 18.04 m/s and 10.48% axial.   

The Table below provides the following information:
•	First row for each maneuver: planned maneuver total delta-V values based on the associated DVTABLEs  
•	Second row for each maneuver: associated final maneuver planning requirements 
•	Third row for each maneuver: predicted velocity error at the time of the maneuver computed by differencing the predicted velocity at the maneuver time (starting with the post-perigee GEONS state prior to the maneuver) vs the definitive GEONS state at the time of the maneuver.
As shown in the table below, all maneuvering spacecraft meet the requirement.
Maneuver ID	Timespan	DVX (m/s)/ 
Req. (m/s)/
DiffVX(m/s)	DVY (m/s)/
Req. (m/s)/
DiffVY(m/s)	DVZ (m/s)/
Req. (m/s)/
DiffVZ(m/s)	
MMS1_GS1470	2023_305/14:54:47 to 2023_305/15:21:37		6.6022	15.0211	5.7345	
		0.066022	0.15021	0.057345	
		0.009784	0.01505	0.007498	
MMS2_GS1470	2023_305/13:04:17 to 2023_305/13:31:37		6.7078	15.299	5.8525	
		0.067078	0.15299	0.058525	
		0.005167	0.01431	0.008724	
MMS3_GS1470	2023_305/09:23:17 to 2023_305/09:51:37		7.0082	15.9423	6.086	
		0.070082	0.159423	0.06086	
		0.009883	0.01548	0.006803	
MMS4_GS1470	2023_305/11:14:17 to 2023_305/11:41:37		6.8412	15.5891	5.9545	
		0.068412	0.155891	0.059545	
		0.002724	0.006751	0.003827