FR1644

Looking at the Restart states from Rev 1645 we have the following results for FR1644
FR1644		NoBurn	Plan	OD	Plan-
NoBurn	OD-NoBurn	Plan-OD	SMA error	PC error	
MMS	Epoch of Plan Apogee	A(km)	A (km)	A (km)	A (km)	A (km)	A (km)			
MMS1	Jul 09 2025 03:31:39	97520.050	97520.050	97520.138	0.000	0.089	-0.089	 		
MMS2	Jul 09 2025 03:32:09	97519.866	97538.940	97539.034	19.073	19.168	-0.095	-0.497%	-2.748%	
MMS3	Jul 09 2025 03:32:04	97520.021	97529.999	97529.918	9.978	9.897	0.081	0.810%	-0.354%	
MMS4	Jul 09 2025 03:31:47	97517.732	97520.791	97520.941	3.059	3.209	-0.150	-4.903%	0.129%	
 
MMS2 was 0.6418 m/s (net delta-v) and 35.04% axial, MMS3 was 0.8536 m/s and 31.22% axial, and MMS4 was 0.8647 m/s and 72.05% axial.
Larger % errors on MMS4 due to maneuver being much smaller than the other two. Note being largely axial, the plane change error for MMS4 was relatively small. There are some significant OD errors which most likely affect the results.

The Table below provides the following information:
•	The start and end times and planned maneuver 
•	Total delta-V (DeltaV_X, DeltaV_Y, and DeltaV_Z) for the first maneuver extracted from the DVTABLE files, 
•	The associated predicted velocity maneuver planning requirement for 1 and 2 orbit predictions (DeltaV_X Req, DeltaV_Y Req, and DeltaV_Z Req)
•	The difference between the predicted velocity and the GEONS definitive velocity at the start time of the first maneuver (Diff_V_X, Diff_V_Y, and Diff_V_Z).Planned maneuver total delta-V values based on the associated DVTABLEs    
As shown in the table below, all meet the requirement except MMS2 DVX, MMS3 DVY, MMS3 DVZ.
Mnvr ID	Time Span	DeltaV_X (m/s)	DeltaV_X Req (m/s)	Diff_V_X (m/s)	DeltaV_Y (m/s)	DeltaV_Y Req (m/s)	Diff_V_Y (m/s)	DeltaV_Z (m/s)	DeltaV_Z Req (m/s)	Diff_V_Z (m/s)	
MMS2	2025_187/22:01:12 to 2025_187/22:02:12	-0.4738	0.01	-0.01286	-0.2117	0.01	-0.0006825	-0.3759	0.01	-0.003019	
MMS4	2025_188/01:26:12 to 2025_188/01:29:12	-0.2358	0.01	-0.006195	0.1353	0.01	0.00167	-0.8182	0.01	0.001306	
MMS3	2025_188/03:01:12 to 2025_188/03:02:32	-0.317	0.01	-0.03354	-0.5765	0.01	-0.02283	-0.5412	0.01	-0.02101